#### Shopping bag

#### Product

Solar Powered Water Pump

Share :

## Solar Powered Water Pump

RM4,100.00

## Available Options

* Options:
Set A - pump water from river
Set B - Pump water from deep well
Set C - Pump water from pond
Set D - Transferring water
* Solar Pole:

Quantity

Contact Us More details
Download Brochure
Description

* Not Included:

1. Piping & Tanki
2. Underground Footing Installation

### Set A - Pump water from river

Items included:

- 550W Surface DC Brushless Pump
- Industrial MPPT Solar Charge Controller
- Solar Panels (800W)
- 2.5m Height Solar Pole x2
- Wiring + Installation

Pump Model Name | PSD3-48550
Max. Power | 550W
Max. Head | 50m
Max. Flow | 3,000 Litres/hour
Outlet | 1” (32mm Pipe)
Daily Water Lift | 2,400 Litres (Cloudy) ~ 4,000 Litres (Sunny)
Title | This is content

Operation:

1. 8.00am ~ 8.30am | Pump Start @ 30% power (volume)
2. 10.30am ~ 2.30pm | Max. Power
3. 6.00pm ~ 6.30pm | Pump Stop
4. Next day resume automatically

* Not Included:

1. Piping & Tanki
2. Underground Footing Installation

### Set B - Pump water from deep well

Items included:

- 400W DC Brushless Pump
- Industrial MPPT Solar Charge Controller
- Solar Panels (600W)
- 30m 2.5mm² Submersible Cable for Pump
- 2.5m Height Solar Pole x1
- Wiring + Installation

Pump Model Name | PSMS-48400
Max. Power | 400W
Max. Head | 50m
Max. Flow | 4,000 Litres/hour
Outlet | 1.25" (32mm Pipe)
Daily Water Lift | 6,000 Litres (Cloudy) 10,000 Litres (Sunny)

Operation:

1. 8.00am ~ 8.30am | Pump Start @ 30% power (volume)
2. 10.30am ~ 2.30pm | Max. Power
3. 6.00pm ~ 6.30pm | Pump Stop
4. Next day resume automatically

* Not Included:

1. Piping & Tanki
2. Underground Footing Installation/ Concrete Works

### Set C - Pump water from pond

Items included:

- 750W Stainless Steel DC Brushless Pump
- Industrial MPPT Solar Charge Controller
- Solar Panels (1250W)
- 2.5m Height Solar Pole x2
- Wiring + Installation

Pump Model Name | PSM3-72750
Max. Power | 750W
Max. Head | 95m
Max. Flow | 4800 Litres/hour
Outlet | 1.25" (32mm Polypipe)
Daily Water Lift | 4,800 Litres (Cloudy) 8,000 Litres (Sunny)

Operation:

1. 8.00am ~ 8.30am | Pump Start @ 30% power (volume)
2. 10.30am ~ 2.30pm | Max. Power
3. 6.00pm ~ 6.30pm | Pump Stop
4. Next day resume automatically

### Set D - Transferring water

3” Sewage Pump Series:

- PSW30-96750-H
- PSW40-1501100-H
- PSW50-1801500-H

Features:

- Latest Permanent Magnet 3-Phase DC Brushless pumps - much more reliable than AC pumps
- Maintenance Free
- Complete with Industrial Weatherproof M PPT Solar Charge Controller
- High Flow Rate
- 3 Overload Protection: Under Load Protection,Lock-Rotor Protection,Thermal Protection
- Optional AC/DC Controller: -AD
  Voltage In:
  PSW40-1501 IOO-AD: AC/ 150-350 DC
  PSW50-1801500-AD: AC/ 180-350 DC

Pump Model Name | PSW30-96750-H | PSW40-1501100-H | PSW50-1801500-H
Voltage | 96V | 150V | 180V
Solar Voltage | 96V ~ 430V | 150V ~ 430V | 180V ~ 430V
Max. Power | 750W | 1100W | 1500W
Max. Flow | 30 M³/hour | 40 M³/hour | 50 M³/hour
Max. Head | 9m | 10m | 10m
Outlet | - | 3" | -
Recommend Solar Power | 200W x6 | 200W x9 | 200W x12

* Specification maybe changed without prior notice

## Solar Powered Water Pump

## You May Also Like

Solar Powered Farmhouse
Shop Product
RM4,999.00
Solar Powered Aerator
Shop Product
RM5,700.00
Solar Powered CCTV
Shop Product
RM1,499.00

© 2026 AGROSMART INDUSTRIES, INC. ALL RIGHT RESERVED.

Web Store by O2O eCommerce

- Terms & Conditions
- Privacy Policy
- Return Policy